|  |  |
| --- | --- |
| Models | One Bay SATA/IDE Turbo NAS |
| Interface/ ports: | USB2.0/ LAN (10/100) |
| LED Display | Power/ Action/ Link |
| Data transfer rate: | Average 8-10 MB/s |
| Supported Server | SAMBA/ FTP/ DHCP/ Printer/ UPnP Media server/Bit torrent (client) |
| Supported Protocol | TCP/IP, USB2.0, |
| Supported Windows O/S | Windows98SE, Me, 2000, XP, Vista / MAC OS X /Linux and Unix(SAMBA/FTP) |
| Support HDD interface: | SATA I/II and IDE (ATA) |
| Support HDD capacity | Up to 2TB |
| Support system file | FAT32 Compatible |
| Single file support | Up to 127GB ( over FAT32 4GB limitation) |
| Product Dimension | 160 (W)x 160(D)x50 (H) mm (main body) |
| Weight | 485 g |
| Operation Environment : | 0 – 35 degree C |
| Storage Environment: | 0 – 50 degree C |
| Certification: | CE, FCC |
| Package contain: | 1x SATA /IDE Turbo NAS 1x RJ45 LAN Cable 1x12V 2A Power supply 1x CD utility ( include user’s manual & SyncQuick™ NAS Manager) |